|  |  |
| --- | --- |
| Consistency | liquid |
| Color | colorless |
| Smell | typical |
| Melting Point | not determined |
| Boiling Point | > 60°C |
| Flash Point | < 19°C |
| Ignition temperature | 200°C (lowest value of the single components) |
| Self flammability | no |
| Danger of explosion | no,but formation of explosive vapors possible |
| Explosion limits | lower 0,6 Vol % upper 15,0 Vol % |
| Vapor pressure @ 20°C | 247 hPa |
| Density (20°C) | 0,798 g/cm³ |
| VOC | 100% |
| Storage time | 12 months |
| Properties | |
| * Thorough cleaning * Rapid Evaporation * High Flash point * Low odor * Special remover for old seals | * Clean and easy removal of a used seals * Makes surfaces oil- and fatfree * Application of a new seal is immediately possible * Deep pore cleaning |
| MARSTON CLEANER is supplied ready. For painting with a brush or a brush. For wiping with a cloth or sponge. By stable flashpoints all AIII products can be easily used in washbasins. | |
| **Packaging** | **Item number** |
| 12 tins á 250 ml | MCL.D250 |
| 10 tins á 1000 ml | MCL.D1000 |
| 10 tins á 10 L | MCL.K10 |
| 12 x spray cans á 400 ml | MCL.Y400 |
| The values are average values. They serve merely for your information, but assume no warranty. | |

MD **MARSTON CLEANER**

18.04.2018